(kicad_pcb
	(version 20260206)
	(generator "synth-eda")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" power)
		(2 "In2.Cu" power)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0)
		(allow_soldermask_bridges_in_footprints yes)
		(trace_min 0.127)
		(clearance_min 0.127)
		(via_min_size 0.6)
		(via_min_drill 0.3)
	)
	(net 0 "")
	(net 1 "net_0")
	(net 2 "net_1")
	(net 3 "net_2")
	(net 4 "net_3")
	(net 5 "net_4")
	(net 6 "net_5")
	(net 7 "net_6")
	(net 8 "net_7")
	(net 9 "net_8")
	(net 10 "net_9")
	(net 11 "net_10")
	(net 12 "net_11")
	(net 13 "net_12")
	(net 14 "net_13")
	(net 15 "net_14")
	(net 16 "net_15")
	(net 17 "net_16")
	(net 18 "net_17")
	(net 19 "net_18")
	(net 20 "net_19")
	(net 21 "net_20")
	(net_class
		"Default"
		"Default net class"
		(clearance 0.127)
		(trace_width 0.127)
		(via_dia 0.6)
		(via_drill 0.3)
		(add_net "net_0")
		(add_net "net_1")
		(add_net "net_2")
		(add_net "net_3")
		(add_net "net_4")
		(add_net "net_6")
		(add_net "net_7")
		(add_net "net_8")
		(add_net "net_9")
		(add_net "net_10")
		(add_net "net_11")
		(add_net "net_12")
		(add_net "net_13")
		(add_net "net_14")
		(add_net "net_15")
		(add_net "net_16")
		(add_net "net_17")
		(add_net "net_18")
		(add_net "net_19")
		(add_net "net_20")
	)
	(net_class
		"Power"
		"Power delivery network"
		(clearance 0.127)
		(trace_width 0.5)
		(via_dia 0.8)
		(via_drill 0.4)
		(add_net "net_5")
	)
	(gr_line
		(start 0 0)
		(end 92.46 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.46 0)
		(end 92.46 53.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.46 53.4)
		(end 0 53.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 53.4)
		(end 0 0)
		(layer "Edge.Cuts")
	)
	(footprint
		"Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12"
		(layer "F.Cu")
		(at 22.32 4.59 180)
		(property
			"Reference"
			"J1"
			(at 0 6.81 180)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"usb_c_receptacle"
			(at 0 -6.81 180)
			(layer "F.Fab")
			(hide yes)
		)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.89 -2.6)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
			(net 0 "")
	)
	(pad "" np_thru_hole circle
		(at 2.89 -2.6)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
			(net 0 "")
	)
	(pad "A1" smd roundrect
		(at -3.25 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "A4" smd roundrect
		(at -2.45 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 1 "net_0")
	)
	(pad "A5" smd roundrect
		(at -1.25 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 3 "net_2")
	)
	(pad "A6" smd roundrect
		(at -0.25 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 20 "net_19")
	)
	(pad "A7" smd roundrect
		(at 0.25 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 21 "net_20")
	)
	(pad "A8" smd roundrect
		(at 1.25 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "A9" smd roundrect
		(at 2.45 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 1 "net_0")
	)
	(pad "A12" smd roundrect
		(at 3.25 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "B1" smd roundrect
		(at 3.25 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "B4" smd roundrect
		(at 2.45 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 1 "net_0")
	)
	(pad "B5" smd roundrect
		(at 1.75 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 4 "net_3")
	)
	(pad "B6" smd roundrect
		(at 0.75 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "B7" smd roundrect
		(at -0.75 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "B8" smd roundrect
		(at -1.75 -4.045)
		(size 0.3 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "B9" smd roundrect
		(at -2.45 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 1 "net_0")
	)
	(pad "B12" smd roundrect
		(at -3.25 -4.045)
		(size 0.6 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "SH" thru_hole oval
		(at -4.32 -3.13)
		(size 1 2.1)
		(drill oval 0.6 1.7)
		(property pad_prop_mechanical)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
			(net 2 "net_1")
	)
	(pad "SH" thru_hole oval
		(at -4.32 1.05)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(property pad_prop_mechanical)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
			(net 2 "net_1")
	)
	(pad "SH" thru_hole oval
		(at 4.32 -3.13)
		(size 1 2.1)
		(drill oval 0.6 1.7)
		(property pad_prop_mechanical)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
			(net 2 "net_1")
	)
	(pad "SH" thru_hole oval
		(at 4.32 1.05)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(property pad_prop_mechanical)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Connector_USB.3dshapes/USB_C_Receptacle_HRO_TYPE-C-31-M-12.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 13.4 20.04)
		(property
			"Reference"
			"U5"
			(at 0 -6.55 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"ams1117_3v3"
			(at 0 6.55 0)
			(layer "F.Fab")
			(hide yes)
		)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.15 -2.3)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "2" smd roundrect
		(at -3.15 0)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 3.15 0)
		(size 2 3.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "3" smd roundrect
		(at -3.15 2.3)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 5 "net_4")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Package_TO_SOT_SMD.3dshapes/SOT-223.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 22.1429 37.6238)
		(property
			"Reference"
			"C1"
			(at 0 -4.48 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0805"
			(at 0 4.48 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 1 "net_0")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 22.2 16.92 180)
		(property
			"Reference"
			"C2"
			(at 0 4.48 180)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0805"
			(at 0 -4.48 180)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 5 "net_4")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 21.48 29.64 90)
		(property
			"Reference"
			"C3"
			(at -5.2 0 -90)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0805"
			(at 5.2 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 15.98 27.67)
		(property
			"Reference"
			"C9"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 5 "net_4")
	)
	(pad "2" smd roundrect
		(at 0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 31.98 4.67)
		(property
			"Reference"
			"R_CC1"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 3 "net_2")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 31.98 9.67)
		(property
			"Reference"
			"R_CC2"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 4 "net_3")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
		(layer "F.Cu")
		(at 22.13 22.57)
		(property
			"Reference"
			"U4"
			(at 0 -5 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"bq24074"
			(at 0 5 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "package/no_lead"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.42 -0.42)
		(size 0.68 0.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "" smd roundrect
		(at -0.42 0.42)
		(size 0.68 0.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "" smd roundrect
		(at 0.42 -0.42)
		(size 0.68 0.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "" smd roundrect
		(at 0.42 0.42)
		(size 0.68 0.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "1" smd roundrect
		(at -1.4625 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "2" smd roundrect
		(at -1.4625 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 7 "net_6")
	)
	(pad "3" smd roundrect
		(at -1.4625 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "4" smd roundrect
		(at -1.4625 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "5" smd roundrect
		(at -0.75 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "6" smd roundrect
		(at -0.25 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "7" smd roundrect
		(at 0.25 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "8" smd roundrect
		(at 0.75 1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "9" smd roundrect
		(at 1.4625 0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "10" smd roundrect
		(at 1.4625 0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 5 "net_4")
	)
	(pad "11" smd roundrect
		(at 1.4625 -0.25)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "12" smd roundrect
		(at 1.4625 -0.75)
		(size 0.825 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 9 "net_8")
	)
	(pad "13" smd roundrect
		(at 0.75 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 1 "net_0")
	)
	(pad "14" smd roundrect
		(at 0.25 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "15" smd roundrect
		(at -0.25 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "16" smd roundrect
		(at -0.75 -1.4625)
		(size 0.25 0.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 8 "net_7")
	)
	(pad "17" smd rect
		(at 0 0)
		(size 1.68 1.68)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Package_DFN_QFN.3dshapes/VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 29.2 19.92 180)
		(property
			"Reference"
			"C4"
			(at 0 4.48 180)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0805"
			(at 0 -4.48 180)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 7 "net_6")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 28.98 14.67)
		(property
			"Reference"
			"R7"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 8 "net_7")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 34.98 14.67)
		(property
			"Reference"
			"R8"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 9 "net_8")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm"
		(layer "F.Cu")
		(at 64.13 33.57)
		(property
			"Reference"
			"U1"
			(at 0 -7.375 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"rp2350"
			(at 0 7.375 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "package/no_lead"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.8 -0.8)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
			(net 0 "")
	)
	(pad "" smd roundrect
		(at -0.8 0.8)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
			(net 0 "")
	)
	(pad "" smd roundrect
		(at 0.8 -0.8)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
			(net 0 "")
	)
	(pad "" smd roundrect
		(at 0.8 0.8)
		(size 1.29 1.29)
		(layers "F.Paste")
		(roundrect_rratio 0.193798)
			(net 0 "")
	)
	(pad "1" smd roundrect
		(at -3.4375 -2.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at -3.4375 -2.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 11 "net_10")
	)
	(pad "3" smd roundrect
		(at -3.4375 -1.8)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 12 "net_11")
	)
	(pad "4" smd roundrect
		(at -3.4375 -1.4)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 14 "net_13")
	)
	(pad "5" smd roundrect
		(at -3.4375 -1)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 15 "net_14")
	)
	(pad "6" smd roundrect
		(at -3.4375 -0.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 13 "net_12")
	)
	(pad "7" smd roundrect
		(at -3.4375 -0.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "8" smd roundrect
		(at -3.4375 0.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "9" smd roundrect
		(at -3.4375 0.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "10" smd roundrect
		(at -3.4375 1)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "11" smd roundrect
		(at -3.4375 1.4)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "12" smd roundrect
		(at -3.4375 1.8)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "13" smd roundrect
		(at -3.4375 2.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "14" smd roundrect
		(at -3.4375 2.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "15" smd roundrect
		(at -2.6 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "16" smd roundrect
		(at -2.2 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "17" smd roundrect
		(at -1.8 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "18" smd roundrect
		(at -1.4 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "19" smd roundrect
		(at -1 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "20" smd roundrect
		(at -0.6 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "21" smd roundrect
		(at -0.2 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "22" smd roundrect
		(at 0.2 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "23" smd roundrect
		(at 0.6 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "24" smd roundrect
		(at 1 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "25" smd roundrect
		(at 1.4 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "26" smd roundrect
		(at 1.8 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 10 "net_9")
	)
	(pad "27" smd roundrect
		(at 2.2 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "28" smd roundrect
		(at 2.6 3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "29" smd roundrect
		(at 3.4375 2.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "30" smd roundrect
		(at 3.4375 2.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "31" smd roundrect
		(at 3.4375 1.8)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "32" smd roundrect
		(at 3.4375 1.4)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "33" smd roundrect
		(at 3.4375 1)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "34" smd roundrect
		(at 3.4375 0.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "35" smd roundrect
		(at 3.4375 0.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "36" smd roundrect
		(at 3.4375 -0.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "37" smd roundrect
		(at 3.4375 -0.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "38" smd roundrect
		(at 3.4375 -1)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "39" smd roundrect
		(at 3.4375 -1.4)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "40" smd roundrect
		(at 3.4375 -1.8)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "41" smd roundrect
		(at 3.4375 -2.2)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "42" smd roundrect
		(at 3.4375 -2.6)
		(size 0.875 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "43" smd roundrect
		(at 2.6 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "44" smd roundrect
		(at 2.2 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "45" smd roundrect
		(at 1.8 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "46" smd roundrect
		(at 1.4 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 21 "net_20")
	)
	(pad "47" smd roundrect
		(at 1 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 20 "net_19")
	)
	(pad "48" smd roundrect
		(at 0.6 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "49" smd roundrect
		(at 0.2 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "50" smd roundrect
		(at -0.2 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "51" smd roundrect
		(at -0.6 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "52" smd roundrect
		(at -1 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "53" smd roundrect
		(at -1.4 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "54" smd roundrect
		(at -1.8 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "55" smd roundrect
		(at -2.2 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "56" smd roundrect
		(at -2.6 -3.4375)
		(size 0.2 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "57" smd rect
		(at 0 0)
		(size 3.2 3.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 72.23 33.42 270)
		(property
			"Reference"
			"C5"
			(at 4.98 0 90)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0603"
			(at -4.98 0 90)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 72.98 38.67 180)
		(property
			"Reference"
			"C6"
			(at 0 4.23 180)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0603"
			(at 0 -4.23 180)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 71.98 43.67)
		(property
			"Reference"
			"R1"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 10 "net_9")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 43.7 13.14)
		(property
			"Reference"
			"U2"
			(at 0 -5.705 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"atecc608"
			(at 0 5.705 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "package/gullwing"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.475 -1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "2" smd roundrect
		(at -2.475 -0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "3" smd roundrect
		(at -2.475 0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "4" smd roundrect
		(at -2.475 1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(pad "5" smd roundrect
		(at 2.475 1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 11 "net_10")
	)
	(pad "6" smd roundrect
		(at 2.475 0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 12 "net_11")
	)
	(pad "7" smd roundrect
		(at 2.475 -0.635)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 0 "")
	)
	(pad "8" smd roundrect
		(at 2.475 -1.905)
		(size 1.95 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 51.98 12.67)
		(property
			"Reference"
			"C7"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.775 0)
		(size 0.9 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 51.98 7.67)
		(property
			"Reference"
			"R2"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 11 "net_10")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 57.98 12.67)
		(property
			"Reference"
			"R3"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 12 "net_11")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"RF_Module:Quectel_BG95-M3"
		(layer "F.Cu")
		(at 66.5 21.94)
		(property
			"Reference"
			"U3"
			(at 0 -6 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"bg95"
			(at 0 6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad
			"32"
			smd
			rect
			(at -1.6 -1.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "net_6")
		)
		(pad
			"3"
			smd
			rect
			(at -1.6 -0.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "net_1")
		)
		(pad
			"35"
			smd
			rect
			(at -1.6 0.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "net_14")
		)
		(pad
			"34"
			smd
			rect
			(at -1.6 1.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "net_13")
		)
		(pad
			"60"
			smd
			rect
			(at 1.6 -1.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "net_15")
		)
		(pad
			"15"
			smd
			rect
			(at 1.6 0.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "net_12")
		)
		(pad
			"17"
			smd
			rect
			(at 1.6 1.5)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "net_18")
		)
		(model
			"${KICAD10_3DMODEL_DIR}/RF_Module.3dshapes/Quectel_BG95-M3.step"
			(at
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint
		"RF_Converter:Johanson_0805"
		(layer "F.Cu")
		(at 74.5 21.94)
		(property
			"Reference"
			"BAL1"
			(at 0 -6 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"balun_2g4"
			(at 0 6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad
			"1"
			smd
			rect
			(at -1.6 -0.8333)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "net_15")
		)
		(pad
			"2"
			smd
			rect
			(at -1.6 0.8333)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "net_16")
		)
		(pad
			"3"
			smd
			rect
			(at 1.6 -0.8333)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "net_17")
		)
		(pad
			"4"
			smd
			rect
			(at 1.6 0.8333)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "net_1")
		)
		(model
			"${KICAD10_3DMODEL_DIR}/RF_Converter.3dshapes/Johanson_0805.step"
			(at
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint
		"Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 73.2 15.92)
		(property
			"Reference"
			"C8"
			(at 0 -4.48 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"c_generic_0805"
			(at 0 4.48 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 7 "net_6")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 42.9834 4.5605)
		(property
			"Reference"
			"R4"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 13 "net_12")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 2 "net_1")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 69.8735 8.9815)
		(property
			"Reference"
			"R5"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 6 "net_5")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 19 "net_18")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(footprint
		"Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 81.98 21.67)
		(property
			"Reference"
			"R6"
			(at 0 -4.23 0)
			(layer "F.SilkS")
		)
		(property
			"Value"
			"r_generic_0603"
			(at 0 4.23 0)
			(layer "F.Fab")
			(hide yes)
		)
	(property "KiLib_Generator" "SMD_2terminal_chip_molded"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 17 "net_16")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.8 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
			(net 18 "net_17")
	)
	(embedded_fonts no)
	(model "/usr/share/kicad/3dmodels/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			yes
			(clearance 0.3)
		)
		(fill
			yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 0)
				(xy 92.46 0)
				(xy 92.46 53.4)
				(xy 0 53.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			yes
			(clearance 0.3)
		)
		(fill
			yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 0)
				(xy 92.46 0)
				(xy 92.46 53.4)
				(xy 0 53.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			yes
			(clearance 0.3)
		)
		(fill
			yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 0)
				(xy 92.46 0)
				(xy 92.46 53.4)
				(xy 0 53.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			yes
			(clearance 0.3)
		)
		(fill
			yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 0)
				(xy 92.46 0)
				(xy 92.46 53.4)
				(xy 0 53.4)
			)
		)
	)
)
